This version is for CVM-8 firmware v1.0 and above.

Send to MIDI port:
Listen on MIDI port:

Show raw inputs: | Show stats: | Show graph:
RX 1 | TX 1 | RX 2 | TX 2 | TX I2C | Conversions
--- | --- | --- | --- | --- | ---

## Configuration Wizard

Eight MIDI CCs | Enable 1: Enable 2: Channel: First CC: Min Voltage: Min Voltage: |
Eight I2C Controllers | Address: First Controller: Min Voltage: Min Voltage: |
MIDI Notes | Enable 1: Enable 2: Channel: Velocity input: 0V Note: |
I2C Notes | Address: Velocity input: 0V Note: |
MIDI Fixed Notes | Enable 1: Enable 2: Channel: Velocity input: First note: |
I2C Fixed Notes | Address: Velocity input: First note: |

## Continuous Generators

|  | MIDI | I2C |
--- | --- | --- | --- | ---
| Input | Enable 1 | Enable 2 | Channel | Message | CC | Min CC | Max CC | Enable | Address | Controller | Min value | Max value | Min Voltage | Max Voltage

## Note Generators

| MIDI | I2C |
--- | --- | --- | ---
| Enable 1 | Enable 2 | Channel | Enable | Address | Pitch Input | Gate Input | Velocity Input | Fixed Pitch | Fixed Velocity | 0V Note | Gate Offset

## Saved Configurations
| DIP switches
--- | ---
| 1 | 2 | 3 | 4
| ## Current Configuration Configuration name:

## Settings

Address (as I2C follower) |

## Bootloader mode

<