This version is for ES-9 firmware v1.3.0 and above.

Send to MIDI port:
Listen on MIDI port:

Choose Config to Upload:
Click to Save Config

Input DC Blocking
Inputs 1/2 | Inputs 3/8 | Inputs 4/5 | Inputs 6/7 | Inputs 9/10 | Inputs 11/12 | Inputs 13/14

Options
S/PDIF Mixer 2

Options
MIDI Thru:

Mixer MIDI channels
USB: DIN:

Sample rate
Unknown

⇩ USB audio ⇩

⇩ Mixer ⇩

⇩ Mixer 2 ⇩

Stereo Links

Mix Smoothing

Macro mix - controls the raw mix below, respecting stereo links

Raw mix - the actual mix matrix running on the hardware

Input EQ

Output DC offsets - can only be applied if a mixer is routed to the output